|  |  |  |  |
| --- | --- | --- | --- |
| Element length (each) | Resonant Freq | SWR |  |
| @ 144 cm | 43 MHz | 1.2 |  |
| @ 140 cm | 44 MHz | 1.2 |  |
| @ 135 cm |  |  |  |

Aluminium tube OD 9 mm

Feed point gap: 1.5 cm

Height above the ground: 48 ft.