|  |  |  |  |
| --- | --- | --- | --- |
| Element length (each) | Resonant Freq @ SWR | Resonant Freq @ SWR | Resonant Freq @ SWR |
| @ 144 cm | 43 MHz @ 1.2 |  |  |
| @ 140 cm | 44 MHz @ 1.2 |  |  |
| @ 135 cm | 47 MHz@ 1.2 |  |  |
| @ 130 cm | 47 MHz @ 1.98 | 54.6 MHz @ 2.171 |  |
|  |  |  |  |

Aluminium tube OD 9 mm

Feed point gap: 1.5 cm

Height above the ground: 48 ft.